**Description, approach, challenge, and improvement**

**Slider switches and LED program**

In this program, we seek to control the LED on the FPGA board with the slider switches. To do this, we must write driver files in assembly that read the inputs from their associated memory addresses. The main processing code is written in C, so we must also include header files that tell the C program to look in external assembly files for the functions called by main.c. In the driver subroutine that reads the switches, we first load a register with the memory address found in the reference manual. Then, we load R0 with the content in that address, thereby returning the “value” the slider switches. Writing to the LED is similar, except that we must write to the memory instead of reading form it. We declare the subroutines “global” to make them visible to the C program.

In the C program, we have a loop that reads the value of the slider-switches. The code directly passes that value to the write\_LEDs\_ASM function.

The header files are simply the signatures of the assembly function in the syntax of C.


An early challenge we had was forgetting to declare the subroutines global for EACH of the subroutines.

**Basic I/O**

This program operates the six seven-segment displays in the following manner:

* The two HEX displays to the left are always “flooded” (i.e. all segments are on).
* The state of the last four slider switches SW3-SW0 will be used to set the value of a number from 0-15, according to its binary number encoding. (ex. “1111” causes “F” to be set).
* The number set by the switches is displayed on the HEX display when the corresponding pushbutton is pressed. For example, pressing the right-most button activates the right-most HEX display. The HEX display remains on even when the pushbutton is no longer pressed. When the button has not been pressed, the HEX display is off.
* Asserting slider switch SW9 “clears” the four right-most HEX displays

To implement this program, we had to first find a way to use the HEX display to display characters 0-9 and A-F. We created two files, HEX\_displays.s and HEX\_displays.h. The second file is a header file that defined an enumeration with values HEX\_0, HEX1…HEX5. Each value is represented by a one-hot encoding at the corresponding position.

These enumerations will be used as inputs to the subroutines HEX\_clear\_ASM, HEX\_flood\_ASM, and HEX\_write\_ASM. They tell the subroutine which HEX display to clear/flood/write. Using one-hot encoding to represent HEX displays allows us to OR multiple HEX displays, pass the resulting value to the subroutines, and clear/flood/write to multiple displays.

The files HEX\_displays.s implements the clear, flood, and write functions in assembly.